UBNT NMS Features – VS – CCPL NMS Features [Base taken as UBNT NMS]

|  |  |  |
| --- | --- | --- |
| Features | UBNT | CCPL |
| Discover devices | Ubiquiti discovery tool.  Discovers Devices within subnets associated to server network interface | No Discovery Tool.  Discovers Devices within subnets associated to server network interface |
| Monitor Device Status | periodically report of runtime status | periodically report of runtime status |
| Firmware update | Yes | Yes |
| View runtime status | Yes | Both for Device and Services |
| Device Grouping | A device tree provides for easy navigation and device selection.  Automatic, static, dynamic grouping | Manual creation of Host parent child relationship. |
| Device activity log/history | Yes | No [Device Based] |
| Access to UI through web | Yes | Yes |
| Mass Firmware Upgrade | Yes | Yes |
| Charts and Graphs | Yes | Yes |
| Tasks Scheduling | Yes | Partial |
| Speed Test | Yes [Agent based] | No |
| Device configuration backup and restore | Yes | No [Planned for Phase 3] |
| Network Map | Automatic | Manual [Planned of Phase 3] |